**Ring Size**

How to measure your ring size

When it comes to choosing a ring, whether for yourself or as a gift for someone else, it’s important to make sure it’s the correct size. In this guide, you’ll find information on how to work out an accurate ring size to ensure a comfortable and secure fit.

Ring size is a measurement that refers to the inside circumference of a ring. Please note that different countries use different standardised systems for indicating the correct ring size, please check what is the corresponding ring size in your country before placing an order.

We are providing information on UK ring sizes and a chart for other countries as a guidance.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Ring Size UK | Inside Diameter (mm) | Inside Circumference (mm) |  USA / Canada | French / Russian | German | Switzerland | Asia |
| A | 11.95 | 37.54 | 1/2 | - | - | - | - |
| A 1/2 | 12.18 | 38.26 | 3/4 | - | - | - | - |
| B | 12.37 | 38.86 | 1 | - | - | - | - |
| B 1/2 | 12.6 | 39.58 | 1 1/4 | - | - | - | - |
| C | 12.78 | 40.15 | 1 1/2 | - | - | - | - |
| C 1/2 | 13 | 40.84 | 1 3/4 | - | - | - | - |
| D | 13.21 | 41.5 | 2 | 41 1/2 | 13 1/2 | 1 1/2 | - |
| D 1/2 | 13.41 | 42.13 | 2 1/4 | - | - | - | - |
| E | 13.61 | 42.76 | 2 1/2 | 42 3/4 | 13 3/4 | 2 3/4 | - |
| E 1/2 | 13.83 | 43.45 | 2 3/4 | - | - | - | - |
| F | 14.05 | 44.14 | 3 | 44 | 14 | 4 | 4 |
| F 1/2 | 14.15 | 44.45 | 3 1/8 | - | - | - | 5 |
| G | 14.36 | 45.11 | 3 1/4 | - | - | - | - |
| G 1/2 | 14.56 | 45.74 | 3 3/8 | 45 1/4 | - | 5 1/4 | 6 |
| H | 14.65 | 46.02 | 3 1/2 | - | 14 1/2 | - | 7 |
| H 1/2 | 14.86 | 46.68 | 3 5/8 | - | - | - | - |
| I | 15.04 | 47.25 | 3 3/4 | 46 1/2 | - | 6 1/2 | 8 |
| I 1/2 | 15.27 | 47.97 | 4 | - | 15 | - | - |
| J | 15.4 | 48.38 | 4 1/4 | 47 3/4 | - | 7 3/4 | 9 |
| J 1/2 | 15.7 | 49.32 | 4 1/2 | - | 15 1/4 | - | - |
| K | 15.8 | 49.64 | 4 5/8 | 49 | 15 1/2 | 9 | 10 |
| K 1/2 | 16 | 50.27 | 4 3/4 | - | - | - | - |
| L | 16.1 | 50.58 | 5 | - | 15 3/4 | - | 11 |
| L 1/2 | 16.41 | 51.55 | 5 1/8 | 50 | - | 10 | 12 |
| M | 16.51 | 51.87 | 5 1/4 | - | - | - | 13 |
| M 1/2 | 16.71 | 52.5 | 5 3/8 | - | - | - | - |
| N | 16.92 | 53.16 | 5 1/2 | 51 3/4 | 16 | 11 3/4 | 14 |
| N 1/2 | 17.13 | 53.82 | 5 3/4 | - | - | - | - |
| O | 17.35 | 54.51 | 5 7/8 | - | - | - | 15 |
| O 1/2 | 17.45 | 54.82 | 6 | 52 3/4 | 16 1/2 | 12 3/4 | - |
| P | 17.75 | 55.76 | 6 1/4 | - | - | - | 16 |
| P 1/2 | 17.97 | 56.45 | 6 1/2 | 54 | 17 | 14 | - |
| Q | 18.19 | 57.15 | 6 3/4 | - | - | - | 17 |
| Q 1/2 | 18.35 | 57.65 | 7 | 55 1/4 | 17 1/4 | 15 1/4 | - |
| R | 18.61 | 58.47 | 7 1/4 | - | - | - | 18 |
| R 1/2 | 18.8 | 59.06 | 7 1/2 | 56 1/2 | 17 3/4 | 16 1/2 | - |
| S | 19.1 | 60 | 7 3/4 | - | - | - | 19 |
| S 1/2 | 19.31 | 60.66 | 8 | 57 3/4 | 18 | 17 3/4 | - |
| T | 19.51 | 61.29 | 8 1/4 | - | - | - | 20 |
| T 1/2 | 19.84 | 62.33 | 8 1/2 | - | 18 1/2 | - | 21 |
| U | 20.02 | 62.89 | 8 5/8 | 59 | - | 19 | 22 |
| U 1/2 | 20.2 | 63.46 | 8 3/4 | - | - | - | - |
| V | 20.32 | 63.84 | 8 7/8 | - | - | - | 23 |
| V 1/2 | 20.68 | 64.97 | 9 | - | 19 | - | - |
| W | 20.76 | 65.22 | 9 1/8 | 60 1/4 | - | 20 1/4 | 24 |
| W 1/2 | 20.94 | 65.78 | 9 1/4 | - | - | - | - |
| X | 21.18 | 66.54 | 9 3/8 | - | - | - | 25 |
| X 1/2 | 21.3 | 66.92 | 9 1/2 | - | 19 1/2 | - | - |
| Y | 21.49 | 67.51 | 9 5/8 | 61 1/2 | - | 21 1/2 | 26 |
| Y 1/2 | 21.69 | 68.14 | 9 3/4 | - | - | - | - |
| Z | 21.89 | 68.77 | 10 | - | 20 | - | 27 |
| Z 1/2 | 22.1 | 69.43 | 10 1/4 | 62 3/4 | - | 22 3/4 | - |